# stream-name: {
# type = rtp|live|ondemand|rtsp
#        rtp = stream originated by an external tool (e.g., gstreamer or
#              ffmpeg) and sent to the plugin via RTP
#        live = local file streamed live to multiple listeners
#               (multiple listeners = same streaming context)
#        ondemand = local file streamed on-demand to a single listener
#                   (multiple listeners = different streaming contexts)
#        rtsp = stream originated by an external RTSP feed (only
#               available if libcurl support was compiled)
# id = <unique numeric ID> (if missing, a random one will be generated)
# description = This is my awesome stream
# is_private = true|false (private streams don't appear when you do a 'list'
#			request)
# secret = <optional password needed for manipulating (e.g., destroying
#			or enabling/disabling) the stream>
# pin = <optional password needed for watching the stream>
# filename = path to the local file to stream (only for live/ondemand)
# audio = true|false (do/don't stream audio)
# video = true|false (do/don't stream video)
#    The following options are only valid for the 'rtp' type:
# data = true|false (do/don't stream text via datachannels)
# audioport = local port for receiving audio frames
# audiortcpport = local port, if any, for receiving and sending audio RTCP feedback
# audiomcast = multicast group port for receiving audio frames, if any
# audioiface = network interface or IP address to bind to, if any (binds to all otherwise)
# audiopt = <audio RTP payload type> (e.g., 111)
# audiortpmap = RTP map of the audio codec (e.g., opus/48000/2)
# audioskew = true|false (whether the plugin should perform skew
#		analisys and compensation on incoming audio RTP stream, EXPERIMENTAL)
# videoport = local port for receiving video frames
# videortcpport = local port, if any, for receiving and sending video RTCP feedback
# videomcast = multicast group port for receiving video frames, if any
# videoiface = network interface or IP address to bind to, if any (binds to all otherwise)
# videopt = <video RTP payload type> (e.g., 100)
# videortpmap = RTP map of the video codec (e.g., VP8/90000)
# videobufferkf = true|false (whether the plugin should store the latest
#		keyframe and send it immediately for new viewers, EXPERIMENTAL)
# videosimulcast = true|false (do|don't enable video simulcasting)
# videoport2 = second local port for receiving video frames (only for rtp, and simulcasting)
# videoport3 = third local port for receiving video frames (only for rtp, and simulcasting)
# videoskew = true|false (whether the plugin should perform skew
#		analisys and compensation on incoming video RTP stream, EXPERIMENTAL)
# videosvc = true|false (whether the video will have SVC support; works only for VP9-SVC, default=false)
# collision = in case of collision (more than one SSRC hitting the same port), the plugin
#		will discard incoming RTP packets with a new SSRC unless this many milliseconds
#		passed, which would then change the current SSRC (0=disabled)
# dataport = local port for receiving data messages to relay
# dataiface = network interface or IP address to bind to, if any (binds to all otherwise)
# databuffermsg = true|false (whether the plugin should store the latest
#		message and send it immediately for new viewers)
# threads = number of threads to assist with the relaying part, which can help
#		if you expect a lot of viewers that may cause the RTP receiving part
#		in the Streaming plugin to slow down and fail to catch up (default=0)
#
# In case you want to use SRTP for your RTP-based mountpoint, you'll need
# to configure the SRTP-related properties as well, namely the suite to
# use for hashing (32 or 80) and the crypto information for decrypting
# the stream (as a base64 encoded string the way SDES does it). Notice
# that with SRTP involved you'll have to pay extra attention to what you
# feed the mountpoint, as you may risk getting SRTP decrypt errors:
# srtpsuite = 32
# srtpcrypto = WbTBosdVUZqEb6Htqhn+m3z7wUh4RJVR8nE15GbN
#
# The following options are only valid for the 'rstp' type:
# url = RTSP stream URL (only for restreaming RTSP)
# rtsp_user = RTSP authorization username (only if type=rtsp)
# rtsp_pwd = RTSP authorization password (only if type=rtsp)
# rtspiface = network interface or IP address to bind to, if any (binds to all otherwise), when receiving RTSP streams
# rtsp_failcheck = whether an error should be returned if connecting to the RTSP server fails (default=true)
#
# Notice that, for 'rtsp' mountpoints, normally the plugin uses the exact
# SDP rtpmap and fmtp attributes the remote camera or RTSP server sent.
# In case the values set remotely are known to conflict with WebRTC viewers,
# you can override both using the settings introduced above.
#
# To test the 'gstreamer-sample' example, check the test_gstreamer.sh
# script in the plugins/streams folder. The live and on-demand  audio
# file streams, use a couple of files (radio.alaw, music.mulaw) that are
# provided in the plugins/streams folder.
#}

general: {
	#admin_key = "supersecret"		# If set, mountpoints can be created via API
									# only if this key is provided in the request
	#rtp_port_range = "20000-40000"	# Range of ports to use for RTP/RTCP when '0' is
									# passed as port for a mountpoint (default=10000-60000)
	#events = false					# Whether events should be sent to event
									# handlers (default=true)
}

#gstreamer-sample: {
	#type = "rtp"
	#id = 1
	#description = "Opus/VP8 live stream coming from gstreamer"
	#audio = true
	#video = true
	#audioport = 5002
	#audiopt = 111
	#audiortpmap = "opus/48000/2"
	#videoport = 5004
	#videopt = 100
	#videortpmap = "VP8/90000"
	#secret = "adminpwd"
#}

#file-live-sample: {
	#type = "live"
	#id = 2
	#description = "a-law file source (radio broadcast)"
	#filename = "/opt/janus/share/janus/streams/radio.alaw"
	#audio = true
	#video = false
	#secret = "adminpwd"
#}

#file-ondemand-sample: {
	#type = "ondemand"
	#id = 3
	#description = "mu-law file source (music)"
	#filename = "/opt/janus/share/janus/streams/music.mulaw"
	#audio = true
	#video = false
	#secret = "adminpwd"
#}

#
# All browsers also support H.264, often through Cisco's OpenH264 plugin.
# The only profile that is definitely supported is the baseline one, which
# means that if you try a higher one it might or might not work. No matter
# which profile you encode, though, you can put a custom one in the SDP if
# you override the fmtp SDP attribute via 'videofmtp'. The following is an
# example of how to create a simple H.264 mountpoint: you can feed it via
# an x264enc+rtph264pay pipeline in gstreamer, an ffmpeg script or other.
#
h264-video: {
	type = "rtsp"
	id = 1
	description = "h264-video"
	enabled = __VIDEO_ENABLED__
	audio = false
	audioiface = "127.0.0.1"
	video = __VIDEO_ENABLED__
        url = "rtsp://127.0.0.1:8554/stream.h264"
	videopt = 96
	videortpmap = "H264/90000"
	videofmtp = "profile-level-id=42e01f;packetization-mode=1"
        data = true
	dataport = 17739
        datatype = "binary"
        dataiface = "127.0.0.1"
        databuffermsg = false
}

#
# The Streaming plugin also supports the broadcasting of datachannel
# messages, either by themselves or along other audio/video streams (e.g.,
# to add a subtitle to a stream you're sending). The following is an
# example of how you can create a datachannel-only mountpoint: you can
# feed it with any tool that can send UDP datagrams, e.g., netcat.
# Notice that the 'rtp' type just indicates this is a live mountpoint:
# datachannel messages will be sent as usual, and not use RTP at all.
#

mjpeg-data: {
	type = "rtp"
	id = 2
	description = "mjpeg-data"
	audio = false
	video = false
	data = true
	dataport = 17740
        datatype = "binary"
	dataiface = "127.0.0.1"
	databuffermsg = false
}

#
# This is a sample configuration for Opus/VP8 multicast streams. You
# need an external script to feed data on those ports, of course.
#
#gstreamer-multicast: {
	#type = "rtp"
	#id = 20
	#description = "Opus/VP8 live multicast stream sample"
	#audio = true
	#video = true
	#audioport = 5002
	#audiomcast = "232.3.4.5"
	#audiopt = 111
	#audiortpmap = "opus/48000/2"
	#videoport = 5004
	#videomcast = "232.3.4.5"
	#videopt = 100
	#videortpmap = "VP8/90000"
#}

#
# This is a sample configuration for an RTSP stream: you can specify
# the url to connect to and whether or not authentication is needed
# using the url/rtsp_user/rtsp_pwd settings (but notice that digest
# authentication will only work if you installed libcurl >= 7.45.0)
# NOTE WELL: the plugin does NOT transcode, so the RTSP stream MUST be
# in a format the browser can digest (e.g., VP8 or H.264 baseline for video)
# Again, you can override payload type, rtpmap and/or fmtp, if needed
#
#rtsp-test: {
	#type = "rtsp"
	#id = 99
	#description = "RTSP Test"
	#audio = false
	#video = true
	#url = "rtsp://127.0.0.1:8554/unicast"
	#rtsp_user = "username"
	#rtsp_pwd = "password"
#}
